ALP1260WV - 12 x 60 W LED Moving Head Waver IP65
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12 INDEPENDENT TILT + ZOOM HEADS - RGBW + AUXILIARY LIGHT - USER MANUAL
Professional IP65 beam, wash and synchronized wave-effect fixture
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READ BEFORE USE  Keep this manual with the fixture. Installation, operation and service must be performed by qualified personnel.
English Edition - Specifications subject to change without notice
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MODEL IDENTIFICATION  This manual is for ALP1260WV. Confirm the model, voltage rating and firmware shown on the actual fixture before installation or programming.
1  Safety Information
DANGER  Disconnect AC power and allow the fixture to cool before opening, cleaning, inspection or service.
This professional fixture must be installed, operated and serviced by qualified personnel.
Use only AC 100-240 V, 50/60 Hz as specified by the technical data and product label. Connect to a protected, properly grounded Class I supply.
Do not operate the fixture with a damaged housing, lens, waterproof connector, mounting point, cable or seal.
After a large temperature change, leave the fixture disconnected until it reaches ambient temperature and all condensation has evaporated.
Do not look directly into the LEDs at close range. Flashing light may trigger seizures in susceptible people; follow local restrictions.
For overhead installation, use rated clamps and an independently rated safety cable attached to the designated point.
Carry the fixture only by its handles or fixed structure. Do not lift it by the moving heads.
Keep ventilation openings clear. Never cover the fixture or operate it near flammable or explosive materials.
IP65 CONDITIONS  IP65 protection applies only when all connector caps, cable glands, covers and seals are correctly fitted and undamaged. IP65 is not an immersion rating. Do not aim high-pressure water jets at the fixture.
2  Product Overview
The ALP1260WV combines twelve independently moving 60 W RGBW heads with motorized zoom and a 432-pixel white/golden-amber auxiliary-light system. It is designed for synchronized wave, beam and wash effects in touring, stage, theatre, studio, club and outdoor-event applications where IP65 protection is required.
2.1 Technical Specifications
	Parameter
	Specification

	Input voltage
	AC 100-240 V, 50/60 Hz

	Rated power
	850 W (source specification)

	Main light source
	12 x 60 W RGBW 4-in-1 LEDs

	Auxiliary light source
	432 x 1 W bi-color LEDs: white + golden amber

	Control
	DMX512 / Auto 1 / Auto 2 / Master-Slave / Sound-active / RDM

	DMX personalities
	26CH / 59CH / 128CH / 152CH / 182CH / 314CH / 329CH

	Dimming
	32-bit, 0-100% linear dimming; selectable response and curves

	Movement / optics
	12 independent tilt and motorized zoom heads

	Primary effects
	Independent wave movement, beam, wash, patterns, color macros and auxiliary-light effects

	Operating temperature
	-30 °C to 50 °C (source specification)

	Strobe
	1-30 Hz

	Firmware update
	Via DMX connection

	Connections
	DMX512 input/output and waterproof power input/output

	Ingress protection
	IP65

	Construction / finish
	Metal, black



2.2 Main Functions
Twelve independently controllable tilt and zoom heads with RGBW color mixing.
White and golden-amber auxiliary LEDs with independent dimming, CTO, strobe and built-in effects.
Built-in tilt macros, color macros, patterns, LED effects and background colors.
Compact shared personalities and expanded per-head personalities up to 329 channels.
RDM support, DMX firmware updating, sound-active operation and synchronized parameter update.
Built-in alignment pins for rapid mechanical joining of compatible fixtures.
3  Setup and Installation
3.1 AC Power
Before connecting power, verify that the product-label voltage and frequency match the local supply. Complete all mounting and data connections before applying power. Keep waterproof connector caps fitted whenever a connector is unused.
3.2 Rigging
STRUCTURAL RATING  The mounting point and every attachment must be rated for at least ten times the fixture load or the higher factor required by local regulations. Keep people clear of the area below during installation and service.
Inspect the fixture, clamps, fasteners, mounting points, safety cable, seals and support structure.
Attach correctly rated clamps to the designated mounting points and tighten all fasteners.
Attach an independently rated safety cable to the designated safety point; never attach it to a moving head or handle.
Confirm clearance for the complete movement and zoom range of all twelve heads.
Recheck every attachment and waterproof connection before applying power.
3.3 DMX512 / RDM Connection
Use shielded, twisted-pair cable intended for RS-485/DMX512. Connect the controller to DMX IN, then link DMX OUT to the next fixture. Assign a unique start address to every independently controlled fixture. RDM requires a compatible controller and bidirectional data equipment.
TERMINATION  At the last fixture in a long or electrically noisy DMX chain, install a 120 ohm resistor between pins 2 and 3 of a male XLR plug and insert it into DMX OUT.
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4  Control Panel and Menu
Use MENU to return, UP/DOWN to select or change a value, and ENTER to open an item or confirm a setting. The display also shows the DMX indicator, error indicator, fixture temperature, address and active personality. Menu labels may vary slightly with firmware revision.
	Menu
	Item
	Option / Range
	Operation

	Address
	DMX Start Address
	001-512
	Set the fixture start address.

	System Settings
	Operating Mode
	DMX / Auto 1 / Auto 2 / Sound
	Select controller, automatic or sound-active operation.

	System Settings
	Channel Mode
	26 / 59 / 128 / 152 / 182 / 314 / 329CH
	Select the DMX personality.

	System Settings
	Pixel Order Reverse
	Off / On
	Reverse the head and pixel sequence.

	System Settings
	Tilt Reverse
	Off / On
	Reverse the tilt direction.

	System Settings
	DMX Hold
	Off / On
	Return to reset state or hold the last DMX frame after signal loss.

	System Settings
	Screen Saver
	Off / On
	Keep the display on or turn it off after inactivity.

	System Settings
	Display Orientation
	Normal / Inverted / Auto
	Set or automatically orient the display.

	System Settings
	Synchronized Update
	Off / On
	Copy settings/calibration to linked fixtures; disconnect the controller first.

	System Settings
	Language
	Chinese / English
	Select the menu language.

	System Settings
	Dimmer Curve
	Linear / Square / Inverse Square / S-Curve
	Select the dimming curve.

	System Settings
	Dimmer Response
	Fast / Smooth
	Select fast or smoothed dimming.

	System Settings
	Head ID
	Off / 1-12
	Service head identification and assignment.

	System Settings
	Factory Reset
	Cancel / Confirm
	Restore factory settings.

	Manual
	Current Personality Channels
	000-255
	Manually test each channel in the selected personality.

	Calibration
	Password
	6688
	Open protected calibration settings.

	Calibration
	Home Position
	Tilt 1-12 / Zoom 1-12, ±127
	Correct mechanical home offsets; record original values first.

	Calibration
	White Balance
	Head 1-12 RGBW, 000-255
	Service-only per-head white-balance calibration; 255 = unchanged.

	Calibration
	Maximum Power
	000-255
	Set the maximum fixture power; 255 = maximum.

	Reset
	Effect / Movement / All
	Confirm
	Reset effect motors, movement motors or the complete fixture.

	Information
	Reset Errors
	Read-only
	View board communication, tilt sensor and zoom reset faults.

	Information
	DMX Monitor
	Read-only
	View received channel values.

	Information
	Sensors
	Read-only
	View zoom Hall, tilt Hall and temperature sensor status.

	Information
	Hardware / Software Version
	Read-only
	View installed hardware and firmware versions.



PROTECTED SETTINGS  Home-position, white-balance, power and head-ID functions are service settings. Record original values before editing; incorrect values can cause positioning faults or abnormal output.
5  DMX512 Channel Reference
Select the same personality on the fixture and controller. Repeated per-head blocks below are written as formulas so every channel remains unambiguous without repeating hundreds of identical rows.
	Personality
	Coverage

	26CH
	Compact shared tilt, zoom, RGBW, effects and auxiliary-light control

	59CH
	Independent tilt/fine and zoom for 12 heads with shared color and auxiliary light

	128CH
	Independent tilt/zoom plus per-head RGBW and two auxiliary colors

	152CH
	Independent tilt/zoom plus per-head RGBW and four auxiliary zones

	182CH
	16-bit RGBW per head plus two auxiliary colors

	314CH
	Maximum per-head tilt, zoom, dimmer, 16-bit RGBW and six auxiliary zones

	329CH
	16-bit shared/per-head color, dimmer, zoom and six auxiliary zones with global auxiliary effects



5.1  26-Channel Personality
Compact shared control of all twelve heads and the auxiliary-light system.
	Channel
	Function
	DMX Value
	Description

	1
	Heads 1-12 Tilt
	000-255
	0-100%

	2
	Heads 1-12 Tilt Fine
	000-255
	Fine adjustment

	3
	Tilt Speed
	000-255
	Fast to slow

	4
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	5
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	6
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	7
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	8
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	9
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	10
	LED Effect Delay
	000-255
	Fast to slow

	11
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	12
	Background Dimmer
	000-255
	0-100%

	13
	Master Dimmer
	000-255
	0-100%

	14
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	15
	Heads 1-12 Zoom
	000-255
	0-100%

	16
	Control
	000-009 / 010-255
	No function / See Control reference

	17
	Red
	000-255
	0-100%

	18
	Green
	000-255
	0-100%

	19
	Blue
	000-255
	0-100%

	20
	White
	000-255
	0-100%

	21
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	22
	Auxiliary White
	000-255
	0-100%

	23
	Auxiliary Golden Amber
	000-255
	0-100%

	24
	Auxiliary CTO
	000-067 / 068-247 / 248-255
	None / CTO / None

	25
	Auxiliary Effect
	000-007 / 008-191 / 192-255
	None / Effect 1-23 / None; 8 values per effect

	26
	Auxiliary Effect Speed
	000-127 / 128-255
	Snap-change slow to fast / Fade slow to fast



5.2  59-Channel Personality
Independent 16-bit tilt and zoom for all heads, with shared main and auxiliary color control.
	Channel
	Function
	DMX Value
	Description

	1-2
	Head 1 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	3-4
	Head 2 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	5-6
	Head 3 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	7-8
	Head 4 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	9-10
	Head 5 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	11-12
	Head 6 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	13-14
	Head 7 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	15-16
	Head 8 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	17-18
	Head 9 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	19-20
	Head 10 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	21-22
	Head 11 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	23-24
	Head 12 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	25
	Tilt Speed
	000-255
	Fast to slow

	26
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	27
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	28
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	29
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	30
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	31
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	32
	LED Effect Delay
	000-255
	Fast to slow

	33
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	34
	Background Dimmer
	000-255
	0-100%

	35
	Master Dimmer
	000-255
	0-100%

	36
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	37-48
	Head 1-12 Zoom
	000-255
	Channel = 36 + head number; 0-100%

	49
	Control
	000-009 / 010-255
	No function / See Control reference

	50
	Red / Cyan
	000-255
	RGBW 0-100% / CMY 100-0%

	51
	Green / Magenta
	000-255
	RGBW 0-100% / CMY 100-0%

	52
	Blue / Yellow
	000-255
	RGBW 0-100% / CMY 100-0%

	53
	White
	000-255
	0-100%

	54
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	55
	Auxiliary White
	000-255
	0-100%

	56
	Auxiliary Golden Amber
	000-255
	0-100%

	57
	Auxiliary CTO
	000-067 / 068-247 / 248-255
	None / CTO / None

	58
	Auxiliary Effect
	000-007 / 008-191 / 192-255
	None / Effect 1-23 / None

	59
	Auxiliary Effect Speed
	000-127 / 128-255
	Snap-change slow to fast / Fade slow to fast



5.3  128-Channel Personality
Per-head RGBW and two auxiliary colors, with independent tilt and zoom.
	Channel
	Function
	DMX Value
	Description

	1-2
	Head 1 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	3-4
	Head 2 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	5-6
	Head 3 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	7-8
	Head 4 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	9-10
	Head 5 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	11-12
	Head 6 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	13-14
	Head 7 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	15-16
	Head 8 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	17-18
	Head 9 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	19-20
	Head 10 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	21-22
	Head 11 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	23-24
	Head 12 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	25
	Tilt Speed
	000-255
	Fast to slow

	26
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	27
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	28
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	29
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	30
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	31
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	32
	LED Effect Delay
	000-255
	Fast to slow

	33
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	34
	Background Dimmer
	000-255
	0-100%

	35
	Master Dimmer
	000-255
	0-100%

	36
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	37
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	38-49
	Head 1-12 Zoom
	000-255
	Channel = 37 + head number; 0-100%

	50
	Control
	000-009 / 010-255
	No function / See Control reference

	51-56
	Shared RGBW + Auxiliary White/Amber
	000-255
	Red, Green, Blue, White, Auxiliary White, Auxiliary Golden Amber

	57-128
	Per-head 6-channel color block
	000-255
	Base = 57 + (head-1) x 6; offsets: R, G, B, W, Aux White, Aux Golden Amber

	57-62
	Head 1 color block
	000-255
	R, G, B, W, Aux White, Aux Golden Amber

	123-128
	Head 12 color block
	000-255
	R, G, B, W, Aux White, Aux Golden Amber



5.4  152-Channel Personality
Per-head RGBW and four auxiliary-light zones, with independent tilt and zoom.
	Channel
	Function
	DMX Value
	Description

	1-2
	Head 1 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	3-4
	Head 2 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	5-6
	Head 3 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	7-8
	Head 4 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	9-10
	Head 5 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	11-12
	Head 6 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	13-14
	Head 7 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	15-16
	Head 8 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	17-18
	Head 9 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	19-20
	Head 10 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	21-22
	Head 11 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	23-24
	Head 12 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	25
	Tilt Speed
	000-255
	Fast to slow

	26
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	27
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	28
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	29
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	30
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	31
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	32
	LED Effect Delay
	000-255
	Fast to slow

	33
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	34
	Background Dimmer
	000-255
	0-100%

	35
	Master Dimmer
	000-255
	0-100%

	36
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	37
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	38-49
	Head 1-12 Zoom
	000-255
	Channel = 37 + head number; 0-100%

	50
	Control
	000-009 / 010-255
	No function / See Control reference

	51-56
	Shared RGBW + Auxiliary White/Amber
	000-255
	Shared color control

	57-152
	Per-head 8-channel color block
	000-255
	Base = 57 + (head-1) x 8; R, G, B, W, Aux White Up, Aux Amber Up, Aux White Down, Aux Amber Down

	57-64
	Head 1 color block
	000-255
	R, G, B, W, four auxiliary zones

	145-152
	Head 12 color block
	000-255
	R, G, B, W, four auxiliary zones



5.5  182-Channel Personality
16-bit per-head RGBW, two auxiliary colors, independent 16-bit tilt and independent zoom.
	Channel
	Function
	DMX Value
	Description

	1-2
	Head 1 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	3-4
	Head 2 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	5-6
	Head 3 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	7-8
	Head 4 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	9-10
	Head 5 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	11-12
	Head 6 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	13-14
	Head 7 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	15-16
	Head 8 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	17-18
	Head 9 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	19-20
	Head 10 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	21-22
	Head 11 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	23-24
	Head 12 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	25
	Tilt Speed
	000-255
	Fast to slow

	26
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	27
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	28
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	29
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	30
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	31
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	32
	LED Effect Delay
	000-255
	Fast to slow

	33
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	34
	Background Dimmer
	000-255
	0-100%

	35
	Background Dimmer Fine
	000-255
	Fine adjustment

	36
	Master Dimmer
	000-255
	0-100%

	37
	Master Dimmer Fine
	000-255
	Fine adjustment

	38
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	39
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	40-51
	Head 1-12 Zoom
	000-255
	Channel = 39 + head number; 0-100%

	52
	Control
	000-009 / 010-255
	No function / See Control reference

	53-60
	Shared RGBW / Fine
	000-255
	R, R Fine, G, G Fine, B, B Fine, W, W Fine

	61-62
	Shared Auxiliary White / Amber
	000-255
	0-100%

	63-182
	Per-head 10-channel color block
	000-255
	Base = 63 + (head-1) x 10; R/R Fine, G/G Fine, B/B Fine, W/W Fine, Aux White, Aux Amber

	63-72
	Head 1 color block
	000-255
	16-bit RGBW plus two auxiliary colors

	173-182
	Head 12 color block
	000-255
	16-bit RGBW plus two auxiliary colors



5.6  314-Channel Personality
Maximum independent control: a 25-channel block for each of the twelve heads.
	Channel
	Function
	DMX Value
	Description

	1
	Control
	000-009 / 010-255
	No function / See Control reference

	2
	Tilt Speed
	000-255
	Fast to slow

	3
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	4
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	5
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	6
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	7
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	8
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	9
	LED Effect Delay
	000-255
	Fast to slow

	10
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	11
	Background Dimmer
	000-255
	0-100%

	12
	Background Dimmer Fine
	000-255
	Fine adjustment

	13
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	14
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	15-314
	Per-head 25-channel block
	000-255
	Base = 15 + (head-1) x 25; Tilt/Fine, Zoom, Dimmer/Fine, RGBW/Fine, six Aux White/Amber zone pairs

	15-39
	Head 1 block
	000-255
	Tilt/Fine, Zoom, Dimmer/Fine, 16-bit RGBW, auxiliary zones 1-6

	290-314
	Head 12 block
	000-255
	Tilt/Fine, Zoom, Dimmer/Fine, 16-bit RGBW, auxiliary zones 1-6



5.7  329-Channel Personality
Expanded shared and per-head 16-bit control with global auxiliary-light effects.
	Channel
	Function
	DMX Value
	Description

	1-2
	Head 1 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	3-4
	Head 2 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	5-6
	Head 3 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	7-8
	Head 4 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	9-10
	Head 5 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	11-12
	Head 6 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	13-14
	Head 7 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	15-16
	Head 8 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	17-18
	Head 9 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	19-20
	Head 10 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	21-22
	Head 11 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	23-24
	Head 12 Tilt / Fine
	000-255
	Coarse 0-100% / fine adjustment

	25
	Tilt Speed
	000-255
	Fast to slow

	26
	Tilt Macro
	000-004 / 005-255
	No function / See Tilt Macro reference

	27
	Color Temperature
	000 / 001-255
	No function / 19,000 K to 2,700 K

	28
	Color Macro
	000 / 001-255
	No function / See Color Macro reference

	29
	Pattern
	000 / 001-255
	No function / Pattern 1-255

	30
	Built-in LED Effect
	000-015 / 016-255
	No function / One effect per 8 values

	31
	LED Effect Speed
	000-127 / 128 / 129-255
	Fast to slow / Stop / Slow to fast

	32
	LED Effect Delay
	000-255
	Fast to slow

	33
	Background Color
	000 / 001-255
	No function / See Color Macro reference

	34
	Background Dimmer
	000-255
	0-100%

	35
	Background Dimmer Fine
	000-255
	Fine adjustment

	36
	Master Dimmer
	000-255
	0-100%

	37
	Master Dimmer Fine
	000-255
	Fine adjustment

	38
	Main Strobe
	000-019 / 020-255
	Off / See Main Strobe reference

	39
	Auxiliary Strobe
	000-255
	See Auxiliary Strobe reference

	40-51
	Head 1-12 Zoom
	000-255
	Channel = 39 + head number; 0-100%

	52
	Control
	000-009 / 010-255
	No function / See Control reference

	53-60
	Shared RGBW / Fine
	000-255
	R/R Fine, G/G Fine, B/B Fine, W/W Fine

	61-324
	Per-head 22-channel block
	000-255
	Base = 61 + (head-1) x 22; Dimmer/Fine, RGBW/Fine, six Aux White/Amber zone pairs

	61-82
	Head 1 block
	000-255
	Dimmer/Fine, 16-bit RGBW and auxiliary zones 1-6

	303-324
	Head 12 block
	000-255
	Dimmer/Fine, 16-bit RGBW and auxiliary zones 1-6

	325
	Global Auxiliary White
	000-255
	0-100%

	326
	Global Auxiliary Golden Amber
	000-255
	0-100%

	327
	Auxiliary CTO
	000-067 / 068-247 / 248-255
	None / CTO / None

	328
	Auxiliary Effect
	000-007 / 008-191 / 192-255
	None / Effect 1-23 / None

	329
	Auxiliary Effect Speed
	000-127 / 128-255
	Snap-change slow to fast / Fade slow to fast



6  Function-Channel Reference
Use these tables whenever a personality row points to a shared macro, strobe or control reference.
6.1  Tilt Macro Ranges
	DMX Value
	Function

	000-004
	No function

	005-009
	Tilt Macro 1

	010-014
	Tilt Macro 2

	015-249
	Tilt Macros 3-49 in consecutive 5-value steps

	250-254
	Tilt Macro 50

	255
	Tilt Macro 51



MACRO OPERATION  When a tilt macro is active, Head 1 Tilt sets the macro start position, Head 1 Tilt Fine sets the swing amplitude, and Tilt Speed sets macro speed. Valid amplitude values are 001-255.
6.2  Color Macro Ranges
	DMX Value
	Function

	000
	No function

	001-002
	White 2700 K

	003-004
	White 3200 K

	005-006
	White 4200 K

	007-008
	White 5600 K

	009-010
	White 8000 K

	011
	Blue

	012-048
	Add Green

	049
	Cyan

	050-086
	Reduce Blue

	087
	Green

	088-124
	Add Red

	125
	Yellow

	126-162
	Reduce Green

	163
	Red

	164-200
	Add Blue

	201
	Magenta

	202-238
	Reduce Red

	239
	Blue

	240-247
	Color fade, fast to slow

	248-255
	Color snap, fast to slow



6.3  Main Strobe Ranges
	DMX Value
	Function

	000-019
	Off

	020-024
	On

	025-064
	Strobe, fast to slow

	065-069
	On

	070-084
	100%-to-0% strobe, fast to slow

	085-089
	On

	090-104
	0%-to-100% strobe, fast to slow

	105-109
	On

	110-124
	Random strobe, fast to slow

	125-129
	On

	130-144
	Random 100%-to-0% strobe, fast to slow

	145-149
	On

	150-164
	Random 0%-to-100% strobe, fast to slow

	165-169
	On

	170-184
	Pulse strobe, fast to slow

	185-189
	On

	190-204
	Random pulse strobe, fast to slow

	205-209
	On

	210-224
	0%-100%-0% strobe, fast to slow

	225-229
	On

	230-244
	Random pulse strobe, fast to slow

	245-255
	On



6.4  Auxiliary Strobe Ranges
	DMX Value
	Function

	000-019
	Blackout

	020-024
	Open

	025-064
	Even strobe, fast to slow

	065-070
	Open

	071-084
	Fast-on / slow-off strobe, slow to fast

	085-089
	Open

	090-104
	Slow-on / fast-off strobe, slow to fast

	105-109
	Open

	110-124
	Random strobe

	125-129
	Open

	130-144
	Random fast-on / slow-off

	145-150
	Open

	151-164
	Random slow-on / fast-off

	165-169
	Open

	170-184
	Strobe program 1

	185-189
	Open

	190-204
	Strobe program 2

	205-209
	Open

	210-224
	Strobe program 3

	225-229
	Open

	230-244
	Strobe program 4

	245-255
	Open



6.5  Control Ranges
	DMX Value
	Function

	000-055
	No function

	056-060
	Tilt motor reset; hold for 5 seconds

	061-065
	Zoom motor reset; hold for 5 seconds

	066-075
	Full fixture reset; hold for 5 seconds

	076-255
	Reserved
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7  Routine Maintenance
ATTENTION  Disconnect AC power and allow the fixture to cool completely before inspection or cleaning.
Inspect the housing, lenses, seals, mounting points, clamps, safety cable, power cable and data connectors before every use.
Replace damaged lenses, cables, covers, connector caps and structural parts before returning the fixture to service.
Clean optical surfaces with a soft, lint-free cloth and suitable optical cleaner; dry every part carefully.
Keep fans and ventilation openings free of dust, fog-fluid residue and obstructions. The source recommends monthly cleaning in dusty environments.
Inspect every tilt and zoom mechanism for unusual noise, resistance, imbalance or positioning errors.
After cleaning or service, confirm that every waterproof seal and connector is correctly refitted before outdoor use.
8  Troubleshooting, RDM and Service
	Symptom
	Check

	No light output
	Verify supply voltage, power connection, circuit protection, dimmer/strobe values and controller output.

	No DMX response after reset
	Confirm DMX mode, start address, selected personality, controller patch, cable polarity and connectors.

	Intermittent or unstable DMX
	Use shielded twisted-pair cable, inspect bidirectional amplifiers, separate signal and high-voltage cables, and terminate the final fixture with 120 ohms.

	Fixture does not start
	Check supply rating, circuit protection, moisture, transport damage and loose connections. Refer internal inspection to qualified service.

	Abnormal tilt or zoom
	Remove obstructions, run the appropriate reset, inspect reversal/ID settings, and refer Hall sensors or mechanisms to qualified service.

	Reduced or unstable output
	Check temperature, ventilation, fan operation, optical cleanliness, supply quality, power calibration and error records.

	DMX works but RDM does not
	Confirm an RDM-compatible controller, bidirectional amplifier and continuity on data pins 2 and 3; all fixtures must remain in DMX mode.



SERVICE  There are no user-serviceable high-voltage parts inside. Refer internal repair, LED-board replacement, motor service, seal replacement and calibration to the manufacturer, its service agent or similarly qualified personnel.
8.1 Warranty and Support
Damage caused by misuse, ignored warnings, unauthorized repair, incorrect installation, compromised waterproof seals or operation outside the specified conditions may be excluded from warranty coverage. Include the model, serial number, firmware version, active personality and a clear fault description when requesting support.
End of manual
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image1.png
| em——
-—em—em—

P—_, S e—— r——)« Pl—-) ?——) —e—— .—) ——— ) ————— )

Trf T LRSS

®






ALP1260WV12x60WLEDMovingHeadWaverIP6512INDEPENDENTTILT+ZOOMHEADS-RGBW+AUXILIARYLIGHT-USERMANUALProfessionalIP65beam,washandsynchronizedwave-effectfixtureREADBEFOREUSEKeepthismanualwiththefixture.Installation,operationandservicemustbeperformedbyqualifiedpersonnel.EnglishEdition-Specificationssubjecttochangewithoutnotice

